**Add Trafficlight ,Button and Buzzer code**

from gpiozero import Button,TrafficLights,Buzzer code

from time import sleep

buzzer=Buzzer(15)

button=Buton(21)

Lights=TrafficLights(25,8,7)

While True :

Button.wait\_for\_press()

Buzzer.on()

Lights.green.on()

Sleep(1)

Lights.green.on()

Sleep(1)

Lights.off()

GPIO.setmode(GPIO.BCM)

Count=0

MAIL\_CHECK\_FREQ=1

RED\_LED=4

GPIO.setup(RED\_LED, GPIO.OUT)

If count==0:

GPIO.output(RED\_LED,False)

Count=1

else:

GPIO.output(RED\_LED,False)